,h1##LENGTH##MILLIMETERS,With Flanges##OTHER##,Use Nominal Diameter##OTHER##,URL##OTHER##,GTIN##OTHER##,GLN##OTHER##,Rings##OTHER##,Ring Visibility##OTHER##,Radius B##LENGTH##MILLIMETERS,Radius A##LENGTH##MILLIMETERS,Pressure Drop##PIPING_PRESSURE##PASCALS,Rings Offset##LENGTH##MILLIMETERS,Handle Offset##LENGTH##MILLIMETERS,K Coefficient##OTHER##,Rings Height##LENGTH##MILLIMETERS,End##OTHER##,Drain Visibility##OTHER##,Drain Handle##OTHER##,Drain Body##OTHER##,Rings Distance##LENGTH##MILLIMETERS,End Distance##LENGTH##MILLIMETERS,Dist D##LENGTH##MILLIMETERS,Dist C##LENGTH##MILLIMETERS,Dist B##LENGTH##MILLIMETERS,Dist A##LENGTH##MILLIMETERS,Connection Diameter##LENGTH##MILLIMETERS,Connector Offset##LENGTH##MILLIMETERS,Air Vent##OTHER##,Geometry Radius##LENGTH##MILLIMETERS,Body Radius##LENGTH##MILLIMETERS,Product Line##OTHER##,Model##OTHER##,Manufacturer URL##OTHER##,Manufacturer Art. No.##OTHER##,Manufacturer##OTHER##,MEPcontent Class##OTHER##,LF##LENGTH##MILLIMETERS,L##LENGTH##MILLIMETERS,Kv##PIPING_FLOW##LITERS_PER_SECOND,IFCExportType##OTHER##,IFCExportAs##OTHER##,H##LENGTH##MILLIMETERS,ETIM Article Class##OTHER##,Valve Distance##LENGTH##MILLIMETERS,Diameter##LENGTH##MILLIMETERS,Description##OTHER##,Custom##OTHER##,Copyright##OTHER##,Content Supplier URL##OTHER##,Connection Outer Diameter##LENGTH##MILLIMETERS,Connection Nominal Diameter##LENGTH##MILLIMETERS,Yellow##OTHER##,Article Type##OTHER##,Article Description##OTHER##,Pressure Stage##OTHER##
HA050F,186,1,1,https://mep.trimble.com,8717811002452,8717811000007,0,1,51,82.5,0,24,138,0,436,0,1,Color RGB 198-000-000,Color RGB 128-128-128,320,74,27,15,3,30,50,175,Color RGB 168-128-048,32,79,Spirotech,HA050F,https://www.spirotech.com/8717811002452,HA050F,Spirotech,SEPARATOR_AIR,350,260,21.39,NOTDEFINED,IfcFilterType,698,EC010260,511,159,Deaerator - Steel- Flange DN50 - High Flow,0,© Trimble Europe BV,www.MEPcontent.com,60.3,50,Color RAL 1003,HA050F,Deaerator - Steel- Flange DN50 - High Flow,PN16
HA050L,186,0,1,https://mep.trimble.com,8717811002445,8717811000007,0,1,51,82.5,0,24,138,0,436,0,1,Color RGB 198-000-000,Color RGB 128-128-128,320,74,27,15,3,30,50,130,Color RGB 168-128-048,32,79,Spirotech,HA050L,https://www.spirotech.com/8717811002445,HA050L,Spirotech,SEPARATOR_AIR,350,260,21.39,NOTDEFINED,IfcFilterType,698,EC010260,511,159,Deaerator - Steel- Weld DN50 - High Flow,0,© Trimble Europe BV,www.MEPcontent.com,60.3,50,Color RAL 1003,HA050L,Deaerator - Steel- Weld DN50 - High Flow,
HA065F,194,1,1,https://mep.trimble.com,8717811002476,8717811000007,0,1,61,92.5,0,24,138,0,436,0,1,Color RGB 198-000-000,Color RGB 128-128-128,320,74,34,15,3,38,65,175,Color RGB 168-128-048,32,79,Spirotech,HA065F,https://www.spirotech.com/8717811002476,HA065F,Spirotech,SEPARATOR_AIR,350,260,34.17,NOTDEFINED,IfcFilterType,698,EC010260,511,159,Deaerator - Steel- Flange DN65 - High Flow,0,© Trimble Europe BV,www.MEPcontent.com,76.1,65,Color RAL 1003,HA065F,Deaerator - Steel- Flange DN65 - High Flow,PN16
HA065L,194,0,1,https://mep.trimble.com,8717811002469,8717811000007,0,1,61,92.5,0,24,138,0,436,0,1,Color RGB 198-000-000,Color RGB 128-128-128,320,74,34,15,3,38,65,130,Color RGB 168-128-048,32,79,Spirotech,HA065L,https://www.spirotech.com/8717811002469,HA065L,Spirotech,SEPARATOR_AIR,350,260,34.17,NOTDEFINED,IfcFilterType,698,EC010260,511,159,Deaerator - Steel- Weld DN65 - High Flow,0,© Trimble Europe BV,www.MEPcontent.com,76.1,65,Color RAL 1003,HA065L,Deaerator - Steel- Weld DN65 - High Flow,
HA080F,213,1,1,https://mep.trimble.com,8717811002490,8717811000007,0,0,69,100,0,35,138,0,436,0,1,Color RGB 198-000-000,Color RGB 128-128-128,320,74,41,17,3,44,80,235,Color RGB 168-128-048,44,109,Spirotech,HA080F,https://www.spirotech.com/8717811002490,HA080F,Spirotech,SEPARATOR_AIR,470,370,45,NOTDEFINED,IfcFilterType,842,EC010260,643,219,Deaerator - Steel- Flange DN80 - High Flow,0,© Trimble Europe BV,www.MEPcontent.com,88.9,80,Color RAL 1003,HA080F,Deaerator - Steel- Flange DN80 - High Flow,PN16
HA080L,213,0,1,https://mep.trimble.com,8717811002483,8717811000007,0,0,69,100,0,35,138,0,436,0,1,Color RGB 198-000-000,Color RGB 128-128-128,320,74,41,17,3,44,80,185,Color RGB 168-128-048,44,109,Spirotech,HA080L,https://www.spirotech.com/8717811002483,HA080L,Spirotech,SEPARATOR_AIR,470,370,45,NOTDEFINED,IfcFilterType,842,EC010260,643,219,Deaerator - Steel- Weld DN80 - High Flow,0,© Trimble Europe BV,www.MEPcontent.com,88.9,80,Color RAL 1003,HA080L,Deaerator - Steel- Weld DN80 - High Flow,
HA100F,225,1,1,https://mep.trimble.com,8717811002513,8717811000007,0,0,79,110,0,35,138,0,436,0,1,Color RGB 198-000-000,Color RGB 128-128-128,320,74,54,17,3,57,100,237,Color RGB 168-128-048,44,109,Spirotech,HA100F,https://www.spirotech.com/8717811002513,HA100F,Spirotech,SEPARATOR_AIR,475,370,71.94,NOTDEFINED,IfcFilterType,842,EC010260,643,219,Deaerator - Steel- Flange DN100 - High Flow,0,© Trimble Europe BV,www.MEPcontent.com,114.3,100,Color RAL 1003,HA100F,Deaerator - Steel- Flange DN100 - High Flow,PN16
HA100L,161,0,1,https://mep.trimble.com,8717811002506,8717811000007,0,0,79,110,0,35,138,0,436,1,0,Color RGB 198-000-000,Color RGB 128-128-128,320,9,54,17,3,57,100,185,Color RGB 168-128-048,44,109,Spirotech,HA100L,https://www.spirotech.com/8717811002506,HA100L,Spirotech,SEPARATOR_AIR,475,370,71.94,NOTDEFINED,IfcFilterType,778,EC010260,579,219,Deaerator - Steel- Weld DN100 - High Flow,0,© Trimble Europe BV,www.MEPcontent.com,114.3,100,Color RAL 1003,HA100L,Deaerator - Steel- Weld DN100 - High Flow,
HA125F,258,1,1,https://mep.trimble.com,8717811002544,8717811000007,0,1,94,125,0,43,300,0,436,0,1,Color RGB 198-000-000,Color RGB 128-128-128,320,74,66,19,3,70,125,317,Color RGB 168-128-048,65,162,Spirotech,HA125F,https://www.spirotech.com/8717811002544,HA125F,Spirotech,SEPARATOR_AIR,635,525,103.06,NOTDEFINED,IfcFilterType,1094,EC010260,873,324,Deaerator - Steel- Flange DN125 - High Flow,0,© Trimble Europe BV,www.MEPcontent.com,139.7,125,Color RAL 1003,HA125F,Deaerator - Steel- Flange DN125 - High Flow,PN16
HA125L,258,0,1,https://mep.trimble.com,8717811002537,8717811000007,0,1,94,125,0,43,300,0,436,0,1,Color RGB 198-000-000,Color RGB 128-128-128,320,74,66,19,3,70,125,262,Color RGB 168-128-048,65,162,Spirotech,HA125L,https://www.spirotech.com/8717811002537,HA125L,Spirotech,SEPARATOR_AIR,635,525,103.06,NOTDEFINED,IfcFilterType,1094,EC010260,873,324,Deaerator - Steel- Weld DN125 - High Flow,0,© Trimble Europe BV,www.MEPcontent.com,139.7,125,Color RAL 1003,HA125L,Deaerator - Steel- Weld DN125 - High Flow,
HA150F,272,1,1,https://mep.trimble.com,8717811002568,8717811000007,0,1,106,129,0,43,300,0,436,0,1,Color RGB 198-000-000,Color RGB 128-128-128,320,74,81,19,3,84,150,317,Color RGB 168-128-048,65,162,Spirotech,HA150F,https://www.spirotech.com/8717811002568,HA150F,Spirotech,SEPARATOR_AIR,635,525,143.89,NOTDEFINED,IfcFilterType,1094,EC010260,873,324,Deaerator - Steel- Flange DN150 - High Flow,0,© Trimble Europe BV,www.MEPcontent.com,168.3,150,Color RAL 1003,HA150F,Deaerator - Steel- Flange DN150 - High Flow,PN16
HA150L,272,0,1,https://mep.trimble.com,8717811002551,8717811000007,0,1,106,129,0,43,300,0,436,0,1,Color RGB 198-000-000,Color RGB 128-128-128,320,74,81,19,3,84,150,262,Color RGB 168-128-048,65,162,Spirotech,HA150L,https://www.spirotech.com/8717811002551,HA150L,Spirotech,SEPARATOR_AIR,635,525,143.89,NOTDEFINED,IfcFilterType,1094,EC010260,873,324,Deaerator - Steel- Weld DN150 - High Flow,0,© Trimble Europe BV,www.MEPcontent.com,168.3,150,Color RAL 1003,HA150L,Deaerator - Steel- Weld DN150 - High Flow,
HA200F,348,1,1,https://mep.trimble.com,8717811002575,8717811000007,0,1,134,170,0,21,296,0,436,0,1,Color RGB 198-000-000,Color RGB 128-128-128,320,74,106,21,3,110,200,387,Color RGB 168-128-048,81,203,Spirotech,HA200F,https://www.spirotech.com/8717811002575,HA200F,Spirotech,SEPARATOR_AIR,775,650,219.72,NOTDEFINED,IfcFilterType,1394,EC010260,1133,406,Deaerator - Steel- Flange DN200 - High Flow,0,© Trimble Europe BV,www.MEPcontent.com,219.1,200,Color RAL 1003,HA200F,Deaerator - Steel- Flange DN200 - High Flow,PN16
HA200L,348,0,1,https://mep.trimble.com,,8717811000007,0,1,134,170,0,21,296,0,436,0,1,Color RGB 198-000-000,Color RGB 128-128-128,320,74,106,21,3,110,200,325,Color RGB 168-128-048,81,203,Spirotech,HA200L,https://www.spirotech.com/products/spirovent/,HA200L,Spirotech,SEPARATOR_AIR,775,650,219.72,NOTDEFINED,IfcFilterType,1394,EC010260,1133,406,Deaerator - Steel- Weld DN200 - High Flow,0,© Trimble Europe BV,www.MEPcontent.com,219.1,200,Color RAL 1003,HA200L,Deaerator - Steel- Weld DN200 - High Flow,
HA250F,441,1,1,https://mep.trimble.com,8717811002599,8717811000007,1,1,160,202.5,0,30,408,0,356,0,1,Color RGB 198-000-000,Color RGB 128-128-128,268,74,133,23,3,136,250,445,Color RGB 168-128-048,102,254,Spirotech,HA250F,https://www.spirotech.com/8717811002599,HA250F,Spirotech,SEPARATOR_AIR,890,750,321.11,NOTDEFINED,IfcFilterType,1806,EC010260,1516,508,Deaerator - Steel- Flange DN250 - High Flow,0,© Trimble Europe BV,www.MEPcontent.com,273,250,Color RAL 1003,HA250F,Deaerator - Steel- Flange DN250 - High Flow,PN16
HA250L,441,0,1,https://mep.trimble.com,,8717811000007,1,1,160,202.5,0,30,408,0,356,0,1,Color RGB 198-000-000,Color RGB 128-128-128,268,74,133,23,3,136,250,375,Color RGB 168-128-048,102,254,Spirotech,HA250L,https://www.spirotech.com/products/spirovent/,HA250L,Spirotech,SEPARATOR_AIR,890,750,321.11,NOTDEFINED,IfcFilterType,1806,EC010260,1516,508,Deaerator - Steel- Weld DN250 - High Flow,0,© Trimble Europe BV,www.MEPcontent.com,273,250,Color RAL 1003,HA250L,Deaerator - Steel- Weld DN250 - High Flow,
HA300F,503,1,1,https://mep.trimble.com,8717811002612,8717811000007,1,1,189,230,0,18,408,0,491,0,1,Color RGB 198-000-000,Color RGB 128-128-128,320,74,158,24,4,162,300,502,Color RGB 168-128-048,122,305,Spirotech,HA300F,https://www.spirotech.com/8717811002612,HA300F,Spirotech,SEPARATOR_AIR,1005,850,427.78,NOTDEFINED,IfcFilterType,2118,EC010260,1796,610,Deaerator - Steel- Flange DN300 - High Flow,0,© Trimble Europe BV,www.MEPcontent.com,323.9,300,Color RAL 1003,HA300F,Deaerator - Steel- Flange DN300 - High Flow,PN16
HA300L,503,0,1,https://mep.trimble.com,,8717811000007,1,1,189,230,0,18,408,0,491,0,1,Color RGB 198-000-000,Color RGB 128-128-128,320,74,158,24,4,162,300,425,Color RGB 168-128-048,122,305,Spirotech,HA300L,https://www.spirotech.com/products/spirovent/,HA300L,Spirotech,SEPARATOR_AIR,1005,850,427.78,NOTDEFINED,IfcFilterType,2118,EC010260,1796,610,Deaerator - Steel- Weld DN300 - High Flow,0,© Trimble Europe BV,www.MEPcontent.com,323.9,300,Color RAL 1003,HA300L,Deaerator - Steel- Weld DN300 - High Flow,
